# Atmel SAM GPIO configuration options

# Copyright (c) 2018 Justin Watson
# Copyright (c) 2020 Gerson Fernando Budke <nandojve@gmail.com>
# SPDX-License-Identifier: Apache-2.0

config GPIO_SAM
	bool "Atmel SAM GPIO (PORT) driver"
	default y
	depends on DT_HAS_ATMEL_SAM_GPIO_ENABLED
	help
	  Enable support for the Atmel SAM 'PORT' GPIO controllers.

config GPIO_SAM4L
	bool "Atmel SAM4L GPIO (PORT) driver"
	default y
	depends on DT_HAS_ATMEL_SAM4L_GPIO_ENABLED
	help
	  Enable support for the Atmel SAM4L 'PORT' GPIO controllers.
