# Copyright (c) 2022, Gerson Fernando Budke <nandojve@gmail.com>
# SPDX-License-Identifier: Apache-2.0

config PINCTRL_SAM
	bool "Atmel SAM pin controller driver"
	default y
	depends on DT_HAS_ATMEL_SAM_PINCTRL_ENABLED
	help
	  Atmel pin controller driver is used on SAM and SAM4L SoC series
